;
; chan_mobile.conf
; configuration file for chan_mobile
;

[general]
interval=30		; Number of seconds between trying to connect to devices.

; The following is a list of adapters we use.
; id must be unique and address is the bdaddr of the adapter from hciconfig.
; Each adapter may only have one device (headset or phone) connected at a time.
; Add an [adapter] entry for each adapter you have.

[adapter]
id=blue
address=00:09:DD:60:01:A3
;forcemaster=yes	; attempt to force adapter into master mode. default is no.
;alignmentdetection=yes ; enable this if you sometimes get 'white noise' on asterisk side of the call
			; its a bug in the bluetooth adapter firmware, enabling this will compensate for it.
			; default is no.

[adapter]
id=dlink
address=00:80:C8:35:52:78

; The following is a list of the devices we deal with.
; Every device listed below will be available for calls in and out of Asterisk.
; Each device needs an adapter=xxxx entry which determines which bluetooth adapter is used.
; Use the CLI command 'mobile search' to discover devices.
; Use the CLI command 'mobile show devices' to see device status.
;
; To place a call out through a mobile phone use Dial(Mobile/[device]/NNN.....) or Dial(Mobile/gn/NNN......) in your dialplan.
; To call a headset use Dial(Mobile/[device]).

[LGTU550]
address=00:E0:91:7F:46:44	; the address of the phone
port=4				; the rfcomm port number (from mobile search)
context=incoming-mobile		; dialplan context for incoming calls
adapter=dlink			; adapter to use
group=1				; this phone is in channel group 1
;sms=no				; support SMS, defaults to yes
;nocallsetup=yes		; set this only if your phone reports that it supports call progress notification, but does not do it. Motorola L6 for example.

[blackberry]
address=00:60:57:32:7E:B2
port=2
context=incoming-mobile
adapter=dlink
group=1
;blackberry=yes			; set this if you are using a blackberry device

[6310i]
address=00:60:57:32:7E:B1
port=13
context=incoming-mobile
adapter=dlink
group=1				; this phone is in channel group 1 also.

[headset]
address=00:0B:9E:11:AE:C6
port=1
type=headset			; This is a headset, not a Phone !
adapter=blue

[headset1]
address=00:0B:9E:11:74:A5
port=1
type=headset
adapter=dlink
