# ChangeLog for asterisk-22.8.0

## Change Log for Release asterisk-22.8.0

### Links:

- Full ChangeLog
- GitHub Diff
- Tarball
- Downloads

### Summary:

- Commits: 57
- Commit Authors: 19
- Issues Resolved: 40
- Security Advisories Resolved: 0

### User Notes:

- #### chan_websocket.conf.sample: Fix category name.

  The category name in the chan_websocket.conf.sample file was incorrect. It should be "global" instead of "general".

- #### cli.c: Allow 'channel request hangup' to accept patterns.

  The 'channel request hangup' CLI command now accepts multiple channel names, POSIX Extended Regular Expressions, glob-like patterns, or a combination of all of them. See the CLI command 'core show help channel request hangup' for full details.

- #### res_sorcery_memory_cache: Reduce cache lock time for sorcery memory cache populate command

  The AMI command sorcery memory cache populate will now return an error if there is an internal error performing the populate. The CLI command will display an error in this case as well.

- #### res_geolocation: Fix multiple issues with XML generation.

  Geolocation: Two new optional profile parameters have been added.

- `pidf_element_id` which sets the value of the `id` attribute on the top-level PIDF-LO `device`, `person` or `tuple` elements.

- `device_id` which sets the content of the `<deviceID>` element. Both parameters can include channel variables.

- #### res_pjsip_messaging: Add support for following 3xx redirects

  A new pjsip endpoint option follow_redirect_methods was added. This option is a comma-delimited, case-insensitive list of SIP methods for which SIP 3XX redirect responses are followed. An alembic upgrade script has been added for adding this new option to the Asterisk database.

- #### taskprocessors: Improve logging and add new cli options

  New CLI command has been added - core show taskprocessor name

- #### ccss: Add option to ccss.conf to globally disable it.

  A new "enabled" parameter has been added to ccss.conf. It defaults to "yes" to preserve backwards compatibility but CCSS is rarely used so setting "enabled = no" in the "general" section can save some unneeded channel locking operations and log message spam. Disabling ccss will also prevent the func_callcompletion and chan_dahdi modules from loading.

- #### Makefile: Add module-list-* targets.

  Try "make module-list-deprecated" to see what modules are on their way out the door.

- #### app_mixmonitor: Add 's' (skip) option to delay recording.

  This change introduces a new 's(<seconds>)' (skip) option to the MixMonitor application. Example: MixMonitor(${UNIQUEID}.wav,s(3)) This skips recording for the first 3 seconds before writing audio to the file. Existing MixMonitor behavior remains unchanged when the 's' option is not used.

- #### app_queue.c: Only announce to head caller if announce_to_first_user

  When announce_to_first_user is false, no announcements are played to the head caller

### Upgrade Notes:

- #### res_geolocation: Fix multiple issues with XML generation.

  Geolocation: In order to correct bugs in both code and documentation, the following changes to the parameters for GML geolocation locations are now in effect:
- The documented but unimplemented `crs` (coordinate reference system) element has been added to the location_info parameter that indicates whether the `2d` or `3d` reference system is to be used. If the crs isn't valid for the shape specified, an error will be generated. The default depends on the shape specified.
- The Circle, Ellipse and ArcBand shapes MUST use a `2d` crs. If crs isn't specified, it will default to `2d` for these shapes. The Sphere, Ellipsoid and Prism shapes MUST use a `3d` crs. If crs isn't specified, it will default to `3d` for these shapes. The Point and Polygon shapes may use either crs. The default crs is `2d` however so if `3d` positions are used, the crs must be explicitly set to `3d`.
- The `geoloc show gml_shape_defs` CLI command has been updated to show which coordinate reference systems are valid for each shape.
- The `pos3d` element has been removed in favor of allowing the `pos` element to include altitude if the crs is `3d`. The number of values in the `pos` element MUST be 2 if the crs is `2d` and 3 if the crs is `3d`. An error will be generated for any other combination.

- The angle unit-of-measure for shapes that use angles should now be included in the respective parameter. The default is `degrees`. There were some inconsistent references to `orientation_uom` in some documentation but that parameter never worked and is now removed. See examples below. Examples... `location_info = shape="Sphere", pos="39.0 -105.0 1620", radius="20" location_info = shape="Point", crs="3d", pos="39.0 -105.0 1620" location_info = shape="Point", pos="39.0 -105.0" location_info = shape=Ellipsoid, pos="39.0 -105.0 1620", semiMajorAxis="20" semiMinorAxis="10", verticalAxis="0", orientation="25 degrees" pidf_element_id = ${CHANNEL(name)}-${EXTEN} device_id = mac:001122334455 Set(GEOLOC_PROFILE(pidf_element_id)=${CHANNEL(name)}/${EXTEN})`

- #### pjsip: Move from threadpool to taskpool

  The threadpool_* options in pjsip.conf have now been deprecated though they continue to be read and used. They have been replaced with taskpool options that give greater control over the underlying taskpool used for PJSIP. An alembic upgrade script has been added to add these options to realtime as well.

- #### app_directed_pickup.c: Change some log messages from NOTICE to VERBOSE.

  In an effort to reduce log spam, two normal progress "pickup attempted" log messages from app_directed_pickup have been changed from NOTICE to VERBOSE(3). This puts them on par with other normal dialplan progress messages.

### Developer Notes:

- #### ccss: Add option to ccss.conf to globally disable it.

  A new API ast_is_cc_enabled() has been added. It should be used to ensure that CCSS is enabled before making any other ast_cc_* calls.

- #### chan_websocket: Add ability to place a MARK in the media stream.

  Apps can now send a `MARK_MEDIA` command with an optional `correlation_id` parameter to chan_websocket which will be placed in the media frame queue. When that frame is dequeued after all intervening media has been played to the core, chan_websocket will send a `MEDIA_MARK_PROCESSED` event to the app with the same correlation_id (if any).

- #### chan_websocket: Add capability for JSON control messages and events.

  The chan_websocket plain-text control and event messages are now deprecated (but remain the default) in favor of JSON formatted messages. See https://docs.asterisk.org/Configuration/Channel-Drivers/WebSocket for more information. A "transport_data" parameter has been added to the

### Commit Authors:

- Alexei Gradinari: (1)
- C. Maj: (1)
- Daouda Taha: (1)
- George Joseph: (12)
- Joe Garlick: (2)
- Joshua C. Colp: (1)
- Justin T. Gibbs: (1)
- Kristian F. Høgh: (1)
- Maximilian Fridrich: (2)
- Michal Hajek: (1)
- Mike Bradeen: (2)
- Nathaniel Wesley Filardo: (1)
- Naveen Albert: (4)
- Peter Krall: (1)
- Sean Bright: (17)
- Sven Kube: (1)
- Tinet-mucw: (2)
- phoneben: (5)
- sarangr7: (1)

## Issue and Commit Detail:

### Closed Issues:

- 60: [bug]: Can't enter any of UTF-8 character in the CLI prompt
- 1417: [bug]: static code analysis issues in abstract_jb
- 1421: [bug]: static code analysis issues in apps/app_dtmfstore.c
- 1427: [bug]: static code analysis issues in apps/app_stream_echo.c
- 1430: [bug]: static code analysis issues in res/stasis/app.c
- 1442: [bug]: static code analysis issues in main/bridge_basic.c
- 1444: [bug]: static code analysis issues in bridges/bridge_simple.c
- 1446: [bug]: static code analysis issues in bridges/bridge_softmix.c
- 1531: [bug]: Memory corruption in manager.c due to double free of criteria variable.
- 1546: [improvement]: Not able to pass the custom variables over the websockets using external Media with ari client library nodejs
- 1552: [improvement]: chan_dahdi.conf.sample: Warnings for callgroup/pickupgroup in stock config
- 1563: [bug]: chan_websocket.c: Wrong variable used in ast_strings_equal() (payload instead of command)
- 1566: [improvement]: Improve Taskprocessor logging
- 1568: [improvement]: Queue is playing announcements when announce_to_first_user is false
- 1572: [improvement]: List modules at various support levels
- 1574: [improvement]: Add playback progress acknowledgment for WebSocket media (per-chunk or byte-level acknowledgment)
- 1576: [improvement]: res_pjsip_messaging: Follow 3xx redirect messages if redirect_method=uri_pjsip
- 1585: [bug]: cli 'stasis show topics' calls a read lock which freezes asterisk till the process is done
- 1587: [bug]: chan_websocket terminates websocket on CNG/non-audio
- 1590: [bug]: Fix: Use ast instead of p->chan to get the DIALSTATUS variable
- 1592: [bug]: app_disa: ResetCDR warning on most invocations
- 1597: [bug]: app_reload: Reload() without arguments doesn't work.
- 1599: [bug]: pbx.c: Running "dialplan reload" shows wrong number of contexts
- 1604: [bug]: asterisk crashes during dtmf input thru websocket -- fixed
- 1609: [bug]: Crash: Double free in ast_channel_destructor leading to SIGABRT (Asterisk 20.17.0) with C++ channel storage
- 1635: [bug]: Regression: Fix endpoint memory leak
- 1638: [bug]: Channel drivers creating ephemeral channels create per-endpoint topics and cache when they shouldn't
- 1643: [bug]: chan_websocket crash when channel hung up before read thread is started
- 1645: [bug]: chan_websocket stuck channels
- 1647: [bug]: "presencestate change" CLI command doesn't accept NOT_SET
- 1648: [bug]: ARI announcer channel can cause crash in specific scenario due to unreffing of borrowed format
- 1660: [bug]: missing hangup cause for ARI ChannelDestroyed when Originated channel times out
- 1662: [improvement]: Include remote IP address in http.c “Requested URI has no handler” log entries
- 1667: [bug]: Multiple geolocation issues with rendering XML
- 1673: [bug]: A crash occurs during the call to mixmonitor_ds_remove_and_free
- 1675: [bug]: res_pjsip_mwi: off-nominal endpoint ao2 reference leak in mwi_get_notify_data()
- 1681: [bug]: stasis/control.c: Memory leak of hangup_time in set-timeout
- 1683: [improvement]: chan_websocket: Use channel FD polling to read data from websocket instead of dedicated thread.
- 1692: [improvement]: Add comment to asterisk.conf.sample clarifying that template sections are ignored
- 1700: [improvement]: Improve sorcery cache populate

### Commits By Author:

- #### Alexei Gradinari (1):

- #### C. Maj (1):

- #### Daouda Taha (1):

- #### George Joseph (12):

- #### Joe Garlick (2):

- #### Joshua C. Colp (1):

- #### Justin T. Gibbs (1):

- #### Kristian F. Høgh (1):

- #### Maximilian Fridrich (2):

- #### Michal Hajek (1):

- #### Mike Bradeen (2):

- #### Nathaniel Wesley Filardo (1):

- #### Naveen Albert (4):

- #### Peter Krall (1):

- #### Sean Bright (17):

- #### Sven Kube (1):

- #### Tinet-mucw (2):

- #### phoneben (5):

- #### sarangr7 (1):

### Commit List:

- chan_websocket.conf.sample: Fix category name.
- chan_websocket: Fixed Ping/Pong messages hanging up the websocket channel
- cli.c: Allow 'channel request hangup' to accept patterns.
- res_sorcery_memory_cache: Reduce cache lock time for sorcery memory cache populate command
- Add comment to asterisk.conf.sample clarifying that template sections are ignored
- chan_websocket: Use the channel's ability to poll fds for the websocket read.
- asterisk.c: Allow multi-byte characters on the Asterisk CLI.
- func_presencestate.c: Allow `NOT_SET` to be set from CLI.
- res/ari/resource_bridges.c: Normalize channel_format ref handling for bridge media
- res_geolocation: Fix multiple issues with XML generation.
- stasis/control.c: Add destructor to timeout_datastore.
- func_talkdetect.c: Remove reference to non-existent variables.
- configure.ac: use AC_PATH_TOOL for nm
- res_pjsip_mwi: Fix off-nominal endpoint ao2 ref leak in mwi_get_notify_data
- res_pjsip_messaging: Add support for following 3xx redirects
- res_pjsip: Introduce redirect module for handling 3xx responses
- app_mixmonitor.c: Fix crash in mixmonitor_ds_remove_and_free when datastore is NULL
- res_pjsip_refer: don't defer session termination for ari transfer
- chan_dahdi.conf.sample: Avoid warnings with default configs.
- main/dial.c: Set channel hangup cause on timeout in handle_timeout_trip
- cel: Add missing manager documentation.
- res_odbc: Use SQL_SUCCEEDED() macro where applicable.
- rtp/rtcp: Configure dual-stack behavior via IPV6_V6ONLY
- http.c: Include remote address in URI handler message.
- pjsip: Move from threadpool to taskpool
- Disable device state caching for ephemeral channels
- chan_websocket: Add locking in send_event and check for NULL websocket handle.
- Fix false null-deref warning in channel_state
- endpoint.c: Plug a memory leak in ast_endpoint_shutdown().
- Revert "func_hangupcause.c: Add access to Reason headers via HANGUPCAUSE()"
- cel_manager.c: Correct manager event mask for CEL events.
- app_queue.c: Update docs to correct QueueMemberPause event name.
- taskprocessors: Improve logging and add new cli options
- manager: fix double free of criteria variable when adding filter
- app_stream_echo.c: Check that stream is non-NULL before dereferencing.
- abstract_jb.c: Remove redundant timer check per static analysis.
- channelstorage_cpp: Fix fallback return value in channelstorage callback
- ccss: Add option to ccss.conf to globally disable it.
- app_directed_pickup.c: Change some log messages from NOTICE to VERBOSE.
- chan_websocket: Fix crash on DTMF_END event.
- chan_websocket.c: Tolerate other frame types
- app_reload: Fix Reload() without arguments.
- pbx.c: Print new context count when reloading dialplan.
- Makefile: Add module-list-* targets.
- app_disa: Avoid use of removed ResetCDR() option.
- core_unreal.c: Use ast instead of p->chan to get the DIALSTATUS variable
- ast_coredumper: Fix multiple issues
- app_mixmonitor: Add 's' (skip) option to delay recording.
- stasis: switch stasis show topics temporary container from list - RBtree
- app_dtmfstore: Avoid a potential buffer overflow.
- main: Explicitly mark case statement fallthrough as such.
- bridge_softmix: Return early on topology allocation failure.
- bridge_simple: Increase code verbosity for clarity.
- app_queue.c: Only announce to head caller if announce_to_first_user
- chan_websocket: Add ability to place a MARK in the media stream.
- chan_websocket: Add capability for JSON control messages and events.
- build: Add menuselect options to facilitate code tracing and coverage

### Commit Details:

#### chan_websocket.conf.sample: Fix category name.

Author: George Joseph Date: 2026-01-21

UserNote: The category name in the chan_websocket.conf.sample file was incorrect. It should be "global" instead of "general".

#### chan_websocket: Fixed Ping/Pong messages hanging up the websocket channel

Author: Joe Garlick Date: 2026-01-15

When chan_websocket received a Ping or a Pong opcode it would cause the channel to hangup. This change allows Ping/Pong opcodes and allows them to silently pass

#### cli.c: Allow 'channel request hangup' to accept patterns.

Author: Sean Bright Date: 2026-01-05

This extends 'channel request hangup' to accept multiple channel names, a POSIX Extended Regular Expression, a glob-like pattern, or a combination of all of them.

UserNote: The 'channel request hangup' CLI command now accepts multiple channel names, POSIX Extended Regular Expressions, glob-like patterns, or a combination of all of them. See the CLI command 'core show help channel request hangup' for full details.

#### res_sorcery_memory_cache: Reduce cache lock time for sorcery memory cache populate command

Author: Mike Bradeen Date: 2026-01-06

Reduce cache lock time for AMI and CLI sorcery memory cache populate commands by adding a new populate_lock to the sorcery_memory_cache struct which is locked separately from the existing cache lock so that the cache lock can be maintained for a reduced time, locking only when the cache objects are removed and re-populated.

Resolves: #1700

UserNote: The AMI command sorcery memory cache populate will now return an error if there is an internal error performing the populate. The CLI command will display an error in this case as well.

#### Add comment to asterisk.conf.sample clarifying that template sections are ignored

Author: phoneben Date: 2026-01-05

Add comment to asterisk.conf.sample clarifying that template sections are ignored.

Resolves: #1692

#### chan_websocket: Use the channel's ability to poll fds for the websocket read.

Author: George Joseph Date: 2025-12-30

We now add the websocket's file descriptor to the channel's fd array and let it poll for data availability instead if having a dedicated thread that does the polling. This eliminates the thread and allows removal of most explicit locking since the core channel code will lock the channel to prevent simultaneous calls to webchan_read, webchan_hangup, etc.

While we were here, the hangup code was refactored to use ast_hangup_with_cause instead of directly queueing an AST_CONTROL_HANGUP frame. This allows us to set hangup causes and generate snapshots.

For a bit of extra debugging, a table of websocket close codes was added to http_websocket.h with an accompanying "to string" function added to res_http_websocket.c

Resolves: #1683

#### asterisk.c: Allow multi-byte characters on the Asterisk CLI.

Author: Sean Bright Date: 2025-12-13

Versions of libedit that support Unicode expect that the EL_GETCFN (the function that does character I/O) will fill in a `wchar_t` with a character, which may be multi-byte. The built-in function that libedit provides, but does not expose with a public API, does properly handle multi-byte sequences.

Due to the design of Asterisk's console processing loop, Asterisk provides its own implementation which does not handle multi-byte characters. Changing Asterisk to use libedit's built-in function would be ideal, but would also require changing some fundamental things about console processing which could be fairly disruptive.

Instead, we bring in libedit's `read_char` implementation and modify it to suit our specific needs.

Resolves: #60

#### func_presencestate.c: Allow `NOT_SET` to be set from CLI.

Author: Sean Bright Date: 2026-01-01

Resolves: #1647

#### res/ari/resource_bridges.c: Normalize channel_format ref handling for bridge media

Author: Peter Krall Date: 2025-12-17

Always take an explicit reference on the format used for bridge playback and recording channels, regardless of where it was sourced, and release it after prepare_bridge_media_channel. This aligns the code paths and avoids mixing borrowed and owned references while preserving behavior.

Fixes: #1648

#### res_geolocation: Fix multiple issues with XML generation.

Author: George Joseph Date: 2025-12-17

- 3d positions were being rendered without an enclosing `<gml:pos>` element resulting in invalid XML.
- There was no way to set the `id` attribute on the enclosing `tuple`, `device` and `person` elements.
- There was no way to set the value of the `deviceID` element.
- Parsing of degree and radian UOMs was broken resulting in them appearing outside an XML element.
- The UOM schemas for degrees and radians were reversed.
- The Ellipsoid shape was missing and the Ellipse shape was defined multiple times.
- The `crs` location_info parameter, although documented, didn't work.
- The `pos3d` location_info parameter appears in some documentation but wasn't being parsed correctly.
- The retransmission-allowed and retention-expiry sub-elements of usage-rules were using the `gp` namespace instead of the `gbp` namespace.

In addition to fixing the above, several other code refactorings were performed and the unit test enhanced to include a round trip XML -> eprofile -> XML validation.

Resolves: #1667

UserNote: Geolocation: Two new optional profile parameters have been added. * `pidf_element_id` which sets the value of the `id` attribute on the top-level PIDF-LO `device`, `person` or `tuple` elements. * `device_id` which sets the content of the `<deviceID>` element. Both parameters can include channel variables.

UpgradeNote: Geolocation: In order to correct bugs in both code and documentation, the following changes to the parameters for GML geolocation locations are now in effect: * The documented but unimplemented `crs` (coordinate reference system) element has been added to the location_info parameter that indicates whether the `2d` or `3d` reference system is to be used. If the crs isn't valid for the shape specified, an error will be generated. The default depends on the shape specified. * The Circle, Ellipse and ArcBand shapes MUST use a `2d` crs. If crs isn't specified, it will default to `2d` for these shapes. The Sphere, Ellipsoid and Prism shapes MUST use a `3d` crs. If crs isn't specified, it will default to `3d` for these shapes. The Point and Polygon shapes may use either crs. The default crs is `2d` however so if `3d` positions are used, the crs must be explicitly set to `3d`. * The `geoloc show gml_shape_defs` CLI command has been updated to show which coordinate reference systems are valid for each shape. * The `pos3d` element has been removed in favor of allowing the `pos` element to include altitude if the crs is `3d`. The number of values in the `pos` element MUST be 2 if the crs is `2d` and 3 if the crs is `3d`. An error will be generated for any other combination. * The angle unit-of-measure for shapes that use angles should now be included in the respective parameter. The default is `degrees`. There were some inconsistent references to `orientation_uom` in some documentation but that parameter never worked and is now removed. See examples below. Examples... `location_info = shape="Sphere", pos="39.0 -105.0 1620", radius="20" location_info = shape="Point", crs="3d", pos="39.0 -105.0 1620" location_info = shape="Point", pos="39.0 -105.0" location_info = shape=Ellipsoid, pos="39.0 -105.0 1620", semiMajorAxis="20" semiMinorAxis="10", verticalAxis="0", orientation="25 degrees" pidf_element_id = ${CHANNEL(name)}-${EXTEN} device_id = mac:001122334455 Set(GEOLOC_PROFILE(pidf_element_id)=${CHANNEL(name)}/${EXTEN})`

#### stasis/control.c: Add destructor to timeout_datastore.

Author: George Joseph Date: 2025-12-31

The timeout_datastore was missing a destructor resulting in a leak of 16 bytes for every outgoing ARI call.

Resolves: #1681

#### func_talkdetect.c: Remove reference to non-existent variables.

Author: Sean Bright Date: 2025-12-30

#### configure.ac: use AC_PATH_TOOL for nm

Author: Nathaniel Wesley Filardo Date: 2025-11-27

`nm` might, especially in cross-compilation scenarios, be available but prefixed with the target triple. So: use `AC_PATH_TOOL` rather than `AC_PATH_PROG` to find it. (See https://www.gnu.org/software/autoconf/manual/autoconf-2.68/html_node/Generic-Programs.html .)

Found and proposed fix tested by cross-compiling Asterisk using Nixpkgs on x86_64 targeting aarch64. :)

#### res_pjsip_mwi: Fix off-nominal endpoint ao2 ref leak in mwi_get_notify_data

Author: Alexei Gradinari Date: 2025-12-29

Delay acquisition of the ast_sip_endpoint reference in mwi_get_notify_data() to avoid an ao2 ref leak on early-return error paths.

Move ast_sip_subscription_get_endpoint() to just before first use so all acquired references are properly cleaned up.

Fixes: #1675

#### res_pjsip_messaging: Add support for following 3xx redirects

Author: Maximilian Fridrich Date: 2025-11-07

This commit integrates the redirect module into res_pjsip_messaging to enable following 3xx redirect responses for outgoing SIP MESSAGEs.

When follow_redirect_methods contains 'message' on an endpoint, Asterisk will now follow 3xx redirect responses for MESSAGEs, similar to how it behaves for INVITE responses.

Resolves: #1576

UserNote: A new pjsip endpoint option follow_redirect_methods was added. This option is a comma-delimited, case-insensitive list of SIP methods for which SIP 3XX redirect responses are followed. An alembic upgrade script has been added for adding this new option to the Asterisk database.

#### res_pjsip: Introduce redirect module for handling 3xx responses

Author: Maximilian Fridrich Date: 2025-11-07

This commit introduces a new redirect handling module that provides infrastructure for following SIP 3xx redirect responses. The redirect functionality respects the endpoint's redirect_method setting and only follows redirects when set to 'uri_pjsip'. This infrastructure can be used by any PJSIP module that needs to handle 3xx redirect responses.

#### app_mixmonitor.c: Fix crash in mixmonitor_ds_remove_and_free when datastore is NULL

Author: Tinet-mucw Date: 2025-12-25

The datastore may be NULL, so a null pointer check needs to be added.

Resolves: #1673

#### res_pjsip_refer: don't defer session termination for ari transfer

Author: Sven Kube Date: 2025-10-23

Allow session termination during an in progress ari handled transfer.

#### chan_dahdi.conf.sample: Avoid warnings with default configs.

Author: Naveen Albert Date: 2025-10-23

callgroup and pickupgroup may only be specified for FXO-signaled channels; however, the chan_dahdi sample config had these options uncommented in the [channels] section, thus applying these settings to all channels, resulting in warnings. Comment these out so there are no warnings with an unmodified sample config.

Resolves: #1552

#### main/dial.c: Set channel hangup cause on timeout in handle_timeout_trip

Author: sarangr7 Date: 2025-12-18

When dial attempts timeout in the core dialing API, the channel's hangup cause was not being set before hanging up. Only the ast_dial_channel structure's internal cause field was updated, but the actual ast_channel hangup cause remained unset.

This resulted in incorrect or missing hangup cause information being reported through CDRs, AMI events, and other mechanisms that read the channel's hangup cause when dial timeouts occurred via applications using the dialing API (FollowMe, Page, etc.).

The fix adds proper channel locking and sets AST_CAUSE_NO_ANSWER on the channel before calling ast_hangup(), ensuring consistent hangup cause reporting across all interfaces.

Resolves: #1660

#### cel: Add missing manager documentation.

Author: Sean Bright Date: 2025-12-12

The LOCAL_OPTIMIZE_BEGIN, STREAM_BEGIN, STREAM_END, and DTMF CEL events were not all documented in the CEL configuration file or the manager documentation for the CEL event.

#### res_odbc: Use SQL_SUCCEEDED() macro where applicable.

Author: Sean Bright Date: 2025-12-17

This is just a cleanup of some repetitive code.

#### rtp/rtcp: Configure dual-stack behavior via IPV6_V6ONLY

Author: Justin T. Gibbs Date: 2025-12-21

Dual-stack behavior (simultaneous listening for IPV4 and IPV6 connections on a single socket) is required by Asterisk's ICE implementation. On systems with the IPV6_V6ONLY sockopt, set the option to 0 (dual-stack enabled) when binding to the IPV6 any address. This ensures correct behavior regardless of the system's default dual-stack configuration.

#### http.c: Include remote address in URI handler message.

Author: Sean Bright Date: 2025-12-22

Resolves: #1662

#### pjsip: Move from threadpool to taskpool

Author: Joshua C. Colp Date: 2025-12-04

This change moves the PJSIP module from the threadpool API to the taskpool API. PJSIP-specific implementations for task usage have been removed and replaced with calls to the optimized taskpool implementations instead. The need for a pool of serializers has also been removed as taskpool inherently provides this. The default settings have also been changed to be more realistic for common usage.

UpgradeNote: The threadpool_* options in pjsip.conf have now been deprecated though they continue to be read and used. They have been replaced with taskpool options that give greater control over the underlying taskpool used for PJSIP. An alembic upgrade script has been added to add these options to realtime as well.

#### Disable device state caching for ephemeral channels

Author: phoneben Date: 2025-12-09

chan_audiosocket/chan_rtp/res_stasis_snoop: Disable device state caching for ephemeral channels

Resolves: #1638

#### chan_websocket: Add locking in send_event and check for NULL websocket handle.

Author: George Joseph Date: 2025-12-10

On an outbound websocket connection, when the triggering caller hangs up, webchan_hangup() closes the outbound websocket session and sets the websocket session handle to NULL. If the hangup happened in the tiny window between opening the outbound websocket connection and before read_thread_handler() was able to send the MEDIA_START message, it could segfault because the websocket session handle was NULL. If it didn't actually segfault, there was also the possibility that the websocket instance wouldn't get cleaned up which could also cause the channel snapshot to not get cleaned up. That could cause memory leaks and `core show channels` to list phantom WebSocket channels.

To prevent the race, the send_event() macro now locks the websocket_pvt instance and checks the websocket session handle before attempting to send the MEDIA_START message.

Resolves: #1643 Resolves: #1645

#### Fix false null-deref warning in channel_state

Author: phoneben Date: 2025-12-08

Resolve analyzer warning in channel_state by checking AST_FLAG_DEAD on snapshot, which is guaranteed non-NULL.

Resolves: #1430

#### endpoint.c: Plug a memory leak in ast_endpoint_shutdown().

Author: George Joseph Date: 2025-12-08

Commit 26795be introduced a memory leak of ast_endpoint when ast_endpoint_shutdown() was called. The leak occurs only if a configuration change removes an endpoint and isn't related to call volume or the length of time asterisk has been running. An ao2_ref(-1) has been added to ast_endpoint_shutdown() to plug the leak.

Resolves: #1635

#### Revert "func_hangupcause.c: Add access to Reason headers via HANGUPCAUSE()"

Author: Sean Bright Date: 2025-12-03

This reverts commit 517766299093d7a9798af68b39951ed8b2469836.

For rationale, see #1621 and #1606

#### cel_manager.c: Correct manager event mask for CEL events.

Author: Sean Bright Date: 2025-12-05

There is no EVENT_FLAG_CEL and these events are raised with as EVENT_FLAG_CALL.

#### app_queue.c: Update docs to correct QueueMemberPause event name.

Author: Sean Bright Date: 2025-12-04

#### taskprocessors: Improve logging and add new cli options

Author: Mike Bradeen Date: 2025-10-28

This change makes some small changes to improve log readability in addition to the following changes:

Modified 'core show taskprocessors' to now show Low time and High time for task execution.

New command 'core show taskprocessor name ' to dump taskprocessor info and current queue.

Addionally, a new test was added to demonstrate the 'show taskprocessor name' functionality: test execute category /main/taskprocessor/ name taskprocessor_cli_show

Setting 'core set debug 3 taskprocessor.c' will now log pushed tasks. (Warning this is will cause extremely high levels of logging at even low traffic levels.)

Resolves: #1566

UserNote: New CLI command has been added - core show taskprocessor name

#### manager: fix double free of criteria variable when adding filter

Author: Michal Hajek Date: 2025-10-13

Signed-off-by: Michal Hajek michal.hajek@daktela.com

Fixes: #1531

#### app_stream_echo.c: Check that stream is non-NULL before dereferencing.

Author: Sean Bright Date: 2025-12-01

Also re-order and rename the arguments of `stream_echo_write_error` to match those of `ast_write_stream` for consistency.

Resolves: #1427

#### abstract_jb.c: Remove redundant timer check per static analysis.

Author: Sean Bright Date: 2025-12-01

While this check is technically unnecessary, it also was not harmful.

The 2 other items mentioned in the linked issue are false positives and require no action.

Resolves: #1417

#### channelstorage_cpp: Fix fallback return value in channelstorage callback

Author: phoneben Date: 2025-11-26

callback returned the last iterated channel when no match existed, causing invalid channel references and potential double frees. Updated to correctly return NULL when there is no match.

Resolves: #1609

#### ccss: Add option to ccss.conf to globally disable it.

Author: George Joseph Date: 2025-11-19

The Call Completion Supplementary Service feature is rarely used but many of it's functions are called by app_dial and channel.c "just in case". These functions lock and unlock the channel just to see if CCSS is enabled on it, which it isn't 99.99% of the time.

UserNote: A new "enabled" parameter has been added to ccss.conf. It defaults to "yes" to preserve backwards compatibility but CCSS is rarely used so setting "enabled = no" in the "general" section can save some unneeded channel locking operations and log message spam. Disabling ccss will also prevent the func_callcompletion and chan_dahdi modules from loading.

DeveloperNote: A new API ast_is_cc_enabled() has been added. It should be used to ensure that CCSS is enabled before making any other ast_cc_* calls.

#### app_directed_pickup.c: Change some log messages from NOTICE to VERBOSE.

Author: George Joseph Date: 2025-11-20

UpgradeNote: In an effort to reduce log spam, two normal progress "pickup attempted" log messages from app_directed_pickup have been changed from NOTICE to VERBOSE(3). This puts them on par with other normal dialplan progress messages.

#### chan_websocket: Fix crash on DTMF_END event.

Author: Sean Bright Date: 2025-11-20

Resolves: #1604

#### chan_websocket.c: Tolerate other frame types

Author: Joe Garlick Date: 2025-11-12

Currently, if chan_websocket receives an un supported frame like comfort noise it will exit the websocket. The proposed change is to tolerate the other frames by not sending them down the websocket but instead just ignoring them.

Resolves: #1587

#### app_reload: Fix Reload() without arguments.

Author: Naveen Albert Date: 2025-11-17

Calling Reload() without any arguments is supposed to reload everything (equivalent to a 'core reload'), but actually does nothing. This is because it was calling ast_module_reload with an empty string, and the argument needs to explicitly be NULL.

Resolves: #1597

#### pbx.c: Print new context count when reloading dialplan.

Author: Naveen Albert Date: 2025-11-17

When running "dialplan reload", the number of contexts reported is initially wrong, as it is the old context count. Running "dialplan reload" a second time returns the correct number of contexts that are loaded. This can confuse users into thinking that the reload didn't work successfully the first time.

This counter is currently only incremented when iterating the old contexts prior to the context merge; at the very end, get the current number of elements in the context hash table and report that instead. This way, the count is correct immediately whenever a reload occurs.

Resolves: #1599

#### Makefile: Add module-list-* targets.

Author: C. Maj Date: 2025-11-17

Convenience wrappers for showing modules at various support levels.

- module-list-core
- module-list-extended
- module-list-deprecated

Resolves: #1572

UserNote: Try "make module-list-deprecated" to see what modules are on their way out the door.

#### app_disa: Avoid use of removed ResetCDR() option.

Author: Naveen Albert Date: 2025-11-14

Commit a46d5f9b760f84b9f27f594b62507c1443aa661b removed the deprecated 'e' option to ResetCDR; this now causes DISA() to emit a warning if attempting to call ResetCDR() with the deprecated option (in all cases except when the no answer option is provided). Rewrite the code to do this the current way.

Resolves: #1592

#### core_unreal.c: Use ast instead of p->chan to get the DIALSTATUS variable

Author: Tinet-mucw Date: 2025-11-13

After p->chan = NULL, ast still points to the valid channel object, using ast safely accesses the channel's DIALSTATUS variable before it's fully destroyed

Resolves: #1590

#### ast_coredumper: Fix multiple issues

Author: George Joseph Date: 2025-11-07

- Fixed an issue with tarball-coredumps when asterisk was invoked without an absolute path.

- Fixed an issue with gdb itself segfaulting when trying to get symbols from separate debuginfo files. The command line arguments needed to be altered such that the gdbinit files is loaded before anything else but the `dump-asterisk` command is run after full initialization.

In the embedded gdbinit script:

- The extract_string_symbol function needed a `char *` cast to work properly.

- The s_strip function needed to be updated to continue to work with the cpp_map_name_id channel storage backend.

- A new function was added to dump the channels when cpp_map_name_id was used.

- The Channel object was updated to account for the new channel storage backends

- The show_locks function was refactored to work correctly.

#### app_mixmonitor: Add 's' (skip) option to delay recording.

Author: Daouda Taha Date: 2025-10-28

The 's' (skip) option delays MixMonitor recording until the specified number of seconds (can be fractional) have elapsed since MixMonitor was invoked.

No audio is written to the recording file during this time. If the call ends before this period, no audio will be saved. This is useful for avoiding early audio such as announcements, ringback tones, or other non-essential sounds.

UserNote: This change introduces a new 's(<seconds>)' (skip) option to the MixMonitor application. Example: MixMonitor(${UNIQUEID}.wav,s(3))

This skips recording for the first 3 seconds before writing audio to the file. Existing MixMonitor behavior remains unchanged when the 's' option is not used.

#### stasis: switch stasis show topics temporary container from list - RBtree

Author: phoneben Date: 2025-11-11

switch stasis show topics temporary container from list to RB-tree minimizing lock time

Resolves: #1585

#### app_dtmfstore: Avoid a potential buffer overflow.

Author: Sean Bright Date: 2025-11-07

Prefer snprintf() so we can readily detect if our output was truncated.

Resolves: #1421

#### main: Explicitly mark case statement fallthrough as such.

Author: Sean Bright Date: 2025-11-07

Resolves: #1442

#### bridge_softmix: Return early on topology allocation failure.

Author: Sean Bright Date: 2025-11-07

Resolves: #1446

#### bridge_simple: Increase code verbosity for clarity.

Author: Sean Bright Date: 2025-11-07

There's no actual problem here, but I can see how it might by confusing.

Resolves: #1444

#### app_queue.c: Only announce to head caller if announce_to_first_user

Author: Kristian F. Høgh Date: 2025-10-30

Only make announcements to head caller if announce_to_first_user is true

Fixes: #1568

UserNote: When announce_to_first_user is false, no announcements are played to the head caller

#### chan_websocket: Add ability to place a MARK in the media stream.

Author: George Joseph Date: 2025-11-05

Also cleaned up a few unused #if blocks, and started sending a few ERROR events back to the apps.

Resolves: #1574

DeveloperNote: Apps can now send a `MARK_MEDIA` command with an optional `correlation_id` parameter to chan_websocket which will be placed in the media frame queue. When that frame is dequeued after all intervening media has been played to the core, chan_websocket will send a `MEDIA_MARK_PROCESSED` event to the app with the same correlation_id (if any).

#### chan_websocket: Add capability for JSON control messages and events.

Author: George Joseph Date: 2025-10-22

With recent enhancements to chan_websocket, the original plain-text implementation of control messages and events is now too limiting. We probably should have used JSON initially but better late than never. Going forward, enhancements that require control message or event changes will only be done to the JSON variants and the plain-text variants are now deprecated but not yet removed.

- Added the chan_websocket.conf config file that allows setting which control message format to use globally: "json" or "plain-text". "plain-text" is the default for now to preserve existing behavior.

- Added a dialstring option `f(json|plain-text)` to allow the format to be overridden on a call-by-call basis. Again, 'plain-text' is the default for now to preserve existing behavior.

The JSON for commands sent by the app to Asterisk must be... `{ "command": "<command>" ... }` where `<command>` is one of `ANSWER`, `HANGUP`, `START_MEDIA_BUFFERING`, etc. The `STOP_MEDIA_BUFFERING` command takes an additional, optional parameter to be returned in the corresponding `MEDIA_BUFFERING_COMPLETED` event: `{ "command": "STOP_MEDIA_BUFFERING", "correlation_id": "<correlation id>" }`.

The JSON for events sent from Asterisk to the app will be... `{ "event": "<event>", "channel_id": "<channel_id>" ... }`. The `MEDIA_START` event will now look like...

`{ "event": "MEDIA_START", "connection_id": "media_connection1", "channel": "WebSocket/media_connection1/0x5140001a0040", "channel_id": "1761245643.1", "format": "ulaw", "optimal_frame_size": 160, "ptime": 20, "channel_variables": { "DIALEDPEERNUMBER": "media_connection1/c(ulaw)", "MEDIA_WEBSOCKET_CONNECTION_ID": "media_connection1", "MEDIA_WEBSOCKET_OPTIMAL_FRAME_SIZE": "160" } }`

Note the addition of the channel variables which can't be supported with the plain-text formatting.

The documentation will be updated with the exact formats for all commands and events.

Resolves: #1546 Resolves: #1563

DeveloperNote: The chan_websocket plain-text control and event messages are now deprecated (but remain the default) in favor of JSON formatted messages. See https://docs.asterisk.org/Configuration/Channel-Drivers/WebSocket for more information.

DeveloperNote: A "transport_data" parameter has been added to the channels/externalMedia ARI endpoint which, for websocket, allows the caller to specify parameters to be added to the dialstring for the channel. For instance, `"transport_data": "f(json)"`.

#### build: Add menuselect options to facilitate code tracing and coverage

Author: George Joseph Date: 2025-10-30

The following options have been added to the menuselect "Compiler Flags" section...

CODE_COVERAGE: The ability to enable code coverage via the `--enable-coverage` configure flag has existed for many years but changing it requires re-running ./configure which is painfully slow. With this commit, you can now enable and disable it via menuselect. Setting this option adds the `-ftest-coverage` and `-fprofile-arcs` flags on the gcc and ld command lines. It also sets DONT_OPTIMIZE. Note: If you use the `--enable-coverage` configure flag, you can't turn it off via menuselect so choose one method and stick to it.

KEEP_FRAME_POINTERS: This option sets `-fno-omit-frame-pointers` on the gcc command line which can facilitate debugging with 'gdb' and tracing with 'perf'. Unlike CODE_COVERAGE, this option doesn't depend on optimization being disabled. It does however conflict with COMPILE_DOUBLE.